**ES7000 & ClearPath Models**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Server** | **Cabinet Door Style** | **Badge Identifier** | **Style Label /**  **Style Identifier** | **Disassembly Instructions** |
| ES7000/One Series  ES7000/600  XPC-L |  |  | MVC-443F  Style names are located  behind cell on left wall.  RAS76004-3BC,  RAS76004-3C,  RAS6001-BAS,  RAS7600401-3BC,  RAS7600401-3C,  RAS600402-POC,  MAR7600401-3C,  MAR6004-POC,  AVA76004-3BC,  AVA76004-3C | End-of-Life Disassembly  Cabinet Level Instructions for Select Models    \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  End-of-Life Disassembly  Instructions for ES7000/One;  ES7000/600; XPC-L |
| ES7000 – 7600R G1, G2, G3, G4 | NA | Various | ES7000 Models:  7600R  7600R G2  7600R G3  7600R G4 |  |
| ClearPath Dorado 3XX,4XX, 7XX, 8XX  Series |  |  | MVC-443F  Style names are located  behind cell on left wall  DOR32041-EXP, DOR38041-EXP, DOR38541-EXP,  DOR70041-AXP, DOR70041-BXP, DOR1-BHS | End-of-Life Disassembly  Cabinet Level Instructions for Select Models    \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  End-of-Life Disassembly  Instructions for Dorado3XX, 4XX, 7XX, 8XX |
| ClearPath Libra 6XX, 7XX, 8XX Series, and  VSE 550 |  | P1010001 | MVC-443F  Style names are located  behind cell on left wall  EDN304-APC, EDN9304-APC,  EDN304-BPC, EDN9304-BPC,  VSE550304-APC | End-of-Life Disassembly  Cabinet Level Instructions for Select Models    \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  End-of-Life Disassembly  Instructions for Libra 6XX; FS1800; VSE 550 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Server** | **Cabinet Door Style** | **Badge Identifier** | **Style Label /**  **Style Identifier** | **Disassembly Instructions** |
| ES7000/500 Series.  ClearPath Libra 5XX,  VSE 500, FS1400, FS1600 |  |  | Style names are located  on front fan assembly  Freestanding cells  CELxxx-F15\*,  CELxxx-F20\*,  CELxxx-V15\*,  CELxxxV20\*  Rack Mounted Cells  CELxxxxx-F15\*,  CELxxxxx-F20\*,  CELxxxxx-V20\*, CELxxxxx-V28  LIB580804-BAS,  LIB581608-BAS,  LIB583216-BAS,  FS141x-xxx  FS160805-BAS,  FS161608-BAS  \* where x =  number representing  processor count,  speed, cache size | End-of-Life Disassembly  Instructions for  ES7000/5XX; Libra 5XX; VSE 500; FS1400; FS1600 |
| ES7000/400 Series |  |  | Style names are located  on rear main assembly  CAS7000405-CR,  CAS7000410-ES,  CAS7000420-GS,  CAS7000430-GD,  CAS7000440-GD,  ACLxxxxxxx-GS\*,  ACLxxxxxxx-GD\*  ACLxxxxxxx-GD2\*, ACLxxxxxxx-GS2\*  \* where x =  number representing processor count,  speed, cache size | End-of-Life Disassembly  Instructions for ES7000/4XX |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Server** | **Cabinet Door Style** | **Badge Identifier** | **Style Label /**  **Style Identifier** | **Disassembly Instructions** |
| ES7000/Classic, ClearPath Dorado 2XX |  |  | Style names are located  on upper left front  cabinet frame assembly  APA1100-BAS,  APA21001-BAS,  APA21002-BAS,  APA2100-BAS,  APA278002-BAS,  APA3016BAS,  APA7120-BAS, CMP7xxxxxxX-GS\*,  CMP7xxxxxxX-GD\*  \*where x =  number representing  processor count,  speed, cache size | End-of-Life Disassembly  Instructions for  Dorado 2XX |

**Dell Based D4x00, D63x0, D83x0, L4x00, L63x0, L83x0 ClearPath Models**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Server** | **Cabinet Door Style** | **Badge Identifier** | **Style Label /**  **Frame Identifier** | **Disassembly Instructions** |
| Dell Servers in 42U Frames |  |  | Style names are located  on upper left front  cabinet frame assembly  RCK4219421-CAB RCK4219422-AXP | End-of-Life Module Disassembly  Instructions for Dell Based Clearpath Systems    See ClearPath Dorado 3XX,4XX, 7XX, 8XX  Series for basic End-of-Life Disassembly  Cabinet Level Instructions |

**ES3000 (Dell Power Edge) Models**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Server** | **Unisys Model Name** | **Dell Equivalent  Model Name** | **Description** | **Disassembly Instructions** |
|  | ES3005 | PE1655MC | Blade Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | Dell Branded Only | PE1900 | 2-socket, Quad-core Tower Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | ES3215L | PE1950 | 2-socket, Quad-core 1U Rack Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | Dell Branded Only | PE1955 | 2-socket, Quad-core Blade Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | ES2026 | PE2500 | 2 processor/5U Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | ES2026L | PE2550 | 2 processor/2U Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | ES3020 | PE2600 | 2 processor/5U Server - XP | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | ES3020L | PE2650 | 2 processor/2U Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | ES3120 | PE2800 | 2 processor/5U Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | ES3120L | PE2850 | 2 processor/2U Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | ES3220 | PE2900 | 2-socket, Quad-core Tower Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | ES3220L | PE2950 | 2-socket, Quad-core 2U Rack Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Server** | **Unisys Model Name** | **Dell Equivalent  Model Name** | **Description** | **Disassembly Instructions** |
|  | ES2046 | PE6400 | 4 Processor Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | ES2046L | PE6450 | 4 Processor Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | ES3040 | PE6600 | 4 Processor/7U Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | ES3040L | PE6650 | 4 Processor/4U Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | ES3140 | PE6800 | Quad Socket, Dual Core Tower Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
|  | ES3140L | PE6850 | Quad Socket, Dual Core 4U Rack Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |

**Other Models**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Server** | **Unisys Model Name** | **Dell Equivalent  Model Name** | **Description** | **Disassembly Instructions** |
| FS1100 | FS111x-xx | PE6600 | SVR:Financial dual Xeon 2.2GHz with 2MB L3 Cache | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
| FS1300 | FS131x3x-xxx | PE6800 | Quad Socket, Dual Core 4U Rack Server | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
| FS1700  Libra 400 | ES3220 | PE2900 | SVR:ES3220 2.83GHz FSB 1333MHZ 2X6M CACHE | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |
| Libra 300 | ES3140 | PE6800 | SVR: dual 3.16GHz with 1MB L3 Cache, or four 3.66 GHz with 1MB L3 Cache | [**Dell PowerEdge Tear-down Instructions**](http://i.dell.com/sites/content/corporate/environment/en/Documents/earth-weee-poweredge-servers.pdf) |